Please include a Justification and make any changes in Red

6.17.10Service Points
The SPNs follow the general method for multi-instance products. Faults are reported with the Instance in the Intermediate Byte (ISB) and a non-zero value in the Most Significant Byte (MSB). These are the allowable Service Points for this DGN (see Table 6.17.10).

Table 6.17.10 — Service Points
	MSB
	ISB
	LSb
	Description

	0
	0-FFh
	0-7
	Node-Global Service Points. Combine the ISB and LSb to calculate. Values from 0-FFh are Standard SPNs – see Table 7.3

	1
	Instance
	0
	Fan

	1
	Instance
	1
	Compressor

	1
	Instance
	2
	Heat Source

	1
	Instance
	3
	Temperature

	1
	Instance
	4
	Outside Air Sensor

	1
	Instance
	5
	Coil Sensor 

	1
	Instance
	6
	No AC Available 

	1
	Instance
	7
	Defrosting

	2
	Instance
	0
	Subnet Communication

	2
	Instance
	1
	Heat Configuration 

	2
	Instance
	2
	Dehumidifier Configuration 

	2
	Instance
	3
	Internal Temperature Sensor

	2
	Instance
	4
	Pressure Switch

	2
	Instance
	5
	Air Flap

	2
	Instance
	6
	Outdoor Coil

	2
	Instance
	7
	Defrost Lockout

	3
	Instance
	0
	DC Voltage

	3
	Instance
	1
	Outdoor Coil Sensor

	3
	Instance
	2
	Compressor Inlet Sensor

	3
	Instance
	3
	Compressor Outlet Sensor

	3
	Instance
	4
	Coil Sensor #2




